Information Center for ARM - EXAMPLE PROJECTS

## Information Center for ARM

## Flashloader for ATMEL

## lowpower

At startup, the program configures all the PIOs as input to avoid parasite consumption (except the UART PIOs). Then a menu is displayed. It is divided into 2 parts. First part allows user to change the configuration (MCK/PCK frequency configuration), The second part allows user to enter in a mode To measure consumption. An amperemeter has to be plugged on the board instead of the VIN jumper. Note for better consumption measurement: - Open JP18 (Potentiometer) before running the program. - Run program out of flash without ICE connected.