SAM3S8/SD8 Software Package: CDC SerialState bits

SAM3S8/SD8 Software Package 1.2
Defines

# CDC SerialState bits
[USB CDC Definitions]

Collaboration diagram for CDC SerialState bits:

## Defines

#define | CDCSerialState_RXDRIVER (1 << 0)
#define | CDCSerialState_TXCARRIER (1 << 1)
#define | CDCSerialState_BREAK (1 << 2)
#define | CDCSerialState_RINGSIGNAL (1 << 3)
#define | CDCSerialState_FRAMING (1 << 4)
#define | CDCSerialState_PARITY (1 << 5)
#define | CDCSerialState_OVERRUN (1 << 6)

## Detailed Description

This page lists the bit map for CDC Serial States.

- CDCSerialState_RXDRIVER
- CDCSerialState_TXCARRIER
- CDCSerialState_BREAK
- CDCSerialState_RINGSIGNAL
- CDCSerialState_FRAMING
- CDCSerialState_PARITY
- CDCSerialState_OVERRUN

## Define Documentation

#define CDCSerialState_BREAK (1 << 2)

Indicates a break has been detected

Definition at line 68 of file CDCNotifications.h.

#define CDCSerialState_FRAMING (1 << 4)

Indicates a framing error has occured

Definition at line 72 of file CDCNotifications.h.

#define CDCSerialState_OVERRUN (1 << 6)

Indicates a data overrun error has occured

Definition at line 76 of file CDCNotifications.h.

#define CDCSerialState_PARITY (1 << 5)

Indicates a parity error has occured

Definition at line 74 of file CDCNotifications.h.

#define CDCSerialState_RINGSIGNAL (1 << 3)

Indicates a ring signal has been detected

Definition at line 70 of file CDCNotifications.h.

#define CDCSerialState_RXDRIVER (1 << 0)

Indicates the receiver carrier signal is present

Definition at line 64 of file CDCNotifications.h.

#define CDCSerialState_TXCARRIER (1 << 1)

Indicates the transmission carrier signal is present

Definition at line 66 of file CDCNotifications.h.

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines