SAM3S8/SD8 Software Package: USB HID Keyboard Device Configure

SAM3S8/SD8 Software Package 1.2
Defines

# USB HID Keyboard Device Configure
[USB Device Framework Configurations]

Collaboration diagram for USB HID Keyboard Device Configure:

## Defines

#define | HIDDKeyboardDriverDescriptors_INTERRUPTIN 1
#define | HIDDKeyboardDriverDescriptors_INTERRUPTIN_POLLING 10
#define | HIDDKeyboardDriverDescriptors_INTERRUPTOUT 2
#define | HIDDKeyboardDriverDescriptors_INTERRUPTOUT_POLLING 10

## Detailed Description

This page lists the defines used by the HID Keyboard Device Driver.

## Endpoint Addresses

- HIDDKeyboardDriverDescriptors_INTERRUPTIN
- HIDDKeyboardDriverDescriptors_INTERRUPTOUT

## Endpoint Polling Rate

- HIDDKeyboardDriverDescriptors_INTERRUPTIN_POLLING
- HIDDKeyboardDriverDescriptors_INTERRUPTOUT_POLLING

## Define Documentation

#define HIDDKeyboardDriverDescriptors_INTERRUPTIN 1

Interrupt IN endpoint number

Definition at line 238 of file USBD_Config.h.

#define HIDDKeyboardDriverDescriptors_INTERRUPTIN_POLLING 10

Interrupt IN endpoint polling rate (in milliseconds)

Definition at line 240 of file USBD_Config.h.

#define HIDDKeyboardDriverDescriptors_INTERRUPTOUT 2

Interrupt OUT endpoint number

Definition at line 242 of file USBD_Config.h.

#define HIDDKeyboardDriverDescriptors_INTERRUPTOUT_POLLING 10

Interrupt OUT endpoint polling rate (in milliseconds)

Definition at line 244 of file USBD_Config.h.

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines