SAM3S8/SD8 Software Package: SBCReadCapacity10 Struct Reference

SAM3S8/SD8 Software Package 1.2
Data Fields

# SBCReadCapacity10 Struct Reference
[USB Massstorage Device Driver]

## Data Fields

unsigned char | bOperationCode
unsigned char | bObsolete1:1
unsigned char | bReserved1:7
unsigned char | pLogicalBlockAddress [4]
unsigned char | pReserved2 [2]
unsigned char | isPMI:1
unsigned char | bReserved3:7
unsigned char | bControl

## Detailed Description

Definition at line 439 of file SBC.h.

## Field Documentation

unsigned char SBCReadCapacity10::bControl

0x00

Definition at line 448 of file SBC.h.

unsigned char SBCReadCapacity10::bObsolete1

Obsolete bit

Definition at line 442 of file SBC.h.

unsigned char SBCReadCapacity10::bOperationCode

0x25 : RBC_READ_CAPACITY

Definition at line 441 of file SBC.h.

unsigned char SBCReadCapacity10::bReserved1

Reserved bits

Definition at line 442 of file SBC.h.

unsigned char SBCReadCapacity10::bReserved3

Reserved bits

Definition at line 446 of file SBC.h.

unsigned char SBCReadCapacity10::isPMI

Partial medium indicator bit

Definition at line 446 of file SBC.h.

unsigned char SBCReadCapacity10::pLogicalBlockAddress[4]

Block to evaluate if PMI is set

Definition at line 444 of file SBC.h.

unsigned char SBCReadCapacity10::pReserved2[2]

Reserved bytes

Definition at line 445 of file SBC.h.

The documentation for this struct was generated from the following file:

- libraries/usb/include/SBC.h

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines