SAM3S8/SD8 Software Package: Peripheral Pio Definitions

SAM3S8/SD8 Software Package 1.2
Defines

# Peripheral Pio Definitions
[SAM3S8 definitions]

Collaboration diagram for Peripheral Pio Definitions:

## Defines

#define | PIO_PA0 (1u << 0)
| Pin Controlled by PA0.
#define | PIO_PA1 (1u << 1)
| Pin Controlled by PA1.
#define | PIO_PA2 (1u << 2)
| Pin Controlled by PA2.
#define | PIO_PA3 (1u << 3)
| Pin Controlled by PA3.
#define | PIO_PA4 (1u << 4)
| Pin Controlled by PA4.
#define | PIO_PA5 (1u << 5)
| Pin Controlled by PA5.
#define | PIO_PA6 (1u << 6)
| Pin Controlled by PA6.
#define | PIO_PA7 (1u << 7)
| Pin Controlled by PA7.
#define | PIO_PA8 (1u << 8)
| Pin Controlled by PA8.
#define | PIO_PA9 (1u << 9)
| Pin Controlled by PA9.
#define | PIO_PA10 (1u << 10)
| Pin Controlled by PA10.
#define | PIO_PA11 (1u << 11)
| Pin Controlled by PA11.
#define | PIO_PA12 (1u << 12)
| Pin Controlled by PA12.
#define | PIO_PA13 (1u << 13)
| Pin Controlled by PA13.
#define | PIO_PA14 (1u << 14)
| Pin Controlled by PA14.
#define | PIO_PA15 (1u << 15)
| Pin Controlled by PA15.
#define | PIO_PA16 (1u << 16)
| Pin Controlled by PA16.
#define | PIO_PA17 (1u << 17)
| Pin Controlled by PA17.
#define | PIO_PA18 (1u << 18)
| Pin Controlled by PA18.
#define | PIO_PA19 (1u << 19)
| Pin Controlled by PA19.
#define | PIO_PA20 (1u << 20)
| Pin Controlled by PA20.
#define | PIO_PA21 (1u << 21)
| Pin Controlled by PA21.
#define | PIO_PA22 (1u << 22)
| Pin Controlled by PA22.
#define | PIO_PA23 (1u << 23)
| Pin Controlled by PA23.
#define | PIO_PA24 (1u << 24)
| Pin Controlled by PA24.
#define | PIO_PA25 (1u << 25)
| Pin Controlled by PA25.
#define | PIO_PA26 (1u << 26)
| Pin Controlled by PA26.
#define | PIO_PA27 (1u << 27)
| Pin Controlled by PA27.
#define | PIO_PA28 (1u << 28)
| Pin Controlled by PA28.
#define | PIO_PA29 (1u << 29)
| Pin Controlled by PA29.
#define | PIO_PA30 (1u << 30)
| Pin Controlled by PA30.
#define | PIO_PA31 (1u << 31)
| Pin Controlled by PA31.
#define | PIO_PB0 (1u << 0)
| Pin Controlled by PB0.
#define | PIO_PB1 (1u << 1)
| Pin Controlled by PB1.
#define | PIO_PB2 (1u << 2)
| Pin Controlled by PB2.
#define | PIO_PB3 (1u << 3)
| Pin Controlled by PB3.
#define | PIO_PB4 (1u << 4)
| Pin Controlled by PB4.
#define | PIO_PB5 (1u << 5)
| Pin Controlled by PB5.
#define | PIO_PB6 (1u << 6)
| Pin Controlled by PB6.
#define | PIO_PB7 (1u << 7)
| Pin Controlled by PB7.
#define | PIO_PB8 (1u << 8)
| Pin Controlled by PB8.
#define | PIO_PB9 (1u << 9)
| Pin Controlled by PB9.
#define | PIO_PB10 (1u << 10)
| Pin Controlled by PB10.
#define | PIO_PB11 (1u << 11)
| Pin Controlled by PB11.
#define | PIO_PB12 (1u << 12)
| Pin Controlled by PB12.
#define | PIO_PB13 (1u << 13)
| Pin Controlled by PB13.
#define | PIO_PB14 (1u << 14)
| Pin Controlled by PB14.
#define | PIO_PC0 (1u << 0)
| Pin Controlled by PC0.
#define | PIO_PC1 (1u << 1)
| Pin Controlled by PC1.
#define | PIO_PC2 (1u << 2)
| Pin Controlled by PC2.
#define | PIO_PC3 (1u << 3)
| Pin Controlled by PC3.
#define | PIO_PC4 (1u << 4)
| Pin Controlled by PC4.
#define | PIO_PC5 (1u << 5)
| Pin Controlled by PC5.
#define | PIO_PC6 (1u << 6)
| Pin Controlled by PC6.
#define | PIO_PC7 (1u << 7)
| Pin Controlled by PC7.
#define | PIO_PC8 (1u << 8)
| Pin Controlled by PC8.
#define | PIO_PC9 (1u << 9)
| Pin Controlled by PC9.
#define | PIO_PC10 (1u << 10)
| Pin Controlled by PC10.
#define | PIO_PC11 (1u << 11)
| Pin Controlled by PC11.
#define | PIO_PC12 (1u << 12)
| Pin Controlled by PC12.
#define | PIO_PC13 (1u << 13)
| Pin Controlled by PC13.
#define | PIO_PC14 (1u << 14)
| Pin Controlled by PC14.
#define | PIO_PC15 (1u << 15)
| Pin Controlled by PC15.
#define | PIO_PC16 (1u << 16)
| Pin Controlled by PC16.
#define | PIO_PC17 (1u << 17)
| Pin Controlled by PC17.
#define | PIO_PC18 (1u << 18)
| Pin Controlled by PC18.
#define | PIO_PC19 (1u << 19)
| Pin Controlled by PC19.
#define | PIO_PC20 (1u << 20)
| Pin Controlled by PC20.
#define | PIO_PC21 (1u << 21)
| Pin Controlled by PC21.
#define | PIO_PC22 (1u << 22)
| Pin Controlled by PC22.
#define | PIO_PC23 (1u << 23)
| Pin Controlled by PC23.
#define | PIO_PC24 (1u << 24)
| Pin Controlled by PC24.
#define | PIO_PC25 (1u << 25)
| Pin Controlled by PC25.
#define | PIO_PC26 (1u << 26)
| Pin Controlled by PC26.
#define | PIO_PC27 (1u << 27)
| Pin Controlled by PC27.
#define | PIO_PC28 (1u << 28)
| Pin Controlled by PC28.
#define | PIO_PC29 (1u << 29)
| Pin Controlled by PC29.
#define | PIO_PC30 (1u << 30)
| Pin Controlled by PC30.
#define | PIO_PC31 (1u << 31)
| Pin Controlled by PC31.
#define | PIO_PA17X1_AD0 (1u << 17)
| Adc signal: AD0.
#define | PIO_PA18X1_AD1 (1u << 18)
| Adc signal: AD1.
#define | PIO_PC13X1_AD10 (1u << 13)
| Adc signal: AD10.
#define | PIO_PC15X1_AD11 (1u << 15)
| Adc signal: AD11.
#define | PIO_PC12X1_AD12 (1u << 12)
| Adc signal: AD12.
#define | PIO_PC29X1_AD13 (1u << 29)
| Adc signal: AD13.
#define | PIO_PC30X1_AD14 (1u << 30)
| Adc signal: AD14.
#define | PIO_PA19X1_AD2_WKUP9 (1u << 19)
| Adc signal: AD2/WKUP9.
#define | PIO_PA20X1_AD3_WKUP10 (1u << 20)
| Adc signal: AD3/WKUP10.
#define | PIO_PB0X1_AD4_RTCOUT0 (1u << 0)
| Adc signal: AD4/RTCOUT0.
#define | PIO_PB1X1_AD5_RTCOUT1 (1u << 1)
| Adc signal: AD5/RTCOUT1.
#define | PIO_PB2X1_AD6_WKUP12 (1u << 2)
| Adc signal: AD6/WKUP12.
#define | PIO_PB3X1_AD7 (1u << 3)
| Adc signal: AD7.
#define | PIO_PA21X1_AD8 (1u << 21)
| Adc signal: AD8.
#define | PIO_PA22X1_AD9 (1u << 22)
| Adc signal: AD9.
#define | PIO_PA8B_ADTRG (1u << 8)
| Adc signal: ADTRG.
#define | PIO_PB13X1_DAC0 (1u << 13)
| Dacc signal: DAC0.
#define | PIO_PB14X1_DAC1 (1u << 14)
| Dacc signal: DAC1.
#define | PIO_PA2C_DATRG (1u << 2)
| Dacc signal: DATRG.
#define | PIO_PC18A_A0 (1u << 18)
| Ebi signal: A0.
#define | PIO_PC19A_A1 (1u << 19)
| Ebi signal: A1.
#define | PIO_PC28A_A10 (1u << 28)
| Ebi signal: A10.
#define | PIO_PC29A_A11 (1u << 29)
| Ebi signal: A11.
#define | PIO_PC30A_A12 (1u << 30)
| Ebi signal: A12.
#define | PIO_PC31A_A13 (1u << 31)
| Ebi signal: A13.
#define | PIO_PA18C_A14 (1u << 18)
| Ebi signal: A14.
#define | PIO_PA19C_A15 (1u << 19)
| Ebi signal: A15.
#define | PIO_PA20C_A16 (1u << 20)
| Ebi signal: A16.
#define | PIO_PA0C_A17 (1u << 0)
| Ebi signal: A17.
#define | PIO_PA1C_A18 (1u << 1)
| Ebi signal: A18.
#define | PIO_PA23C_A19 (1u << 23)
| Ebi signal: A19.
#define | PIO_PC20A_A2 (1u << 20)
| Ebi signal: A2.
#define | PIO_PA24C_A20 (1u << 24)
| Ebi signal: A20.
#define | PIO_PC16A_A21_NANDALE (1u << 16)
| Ebi signal: A21/NANDALE.
#define | PIO_PC17A_A22_NANDCLE (1u << 17)
| Ebi signal: A22/NANDCLE.
#define | PIO_PA25C_A23 (1u << 25)
| Ebi signal: A23.
#define | PIO_PC21A_A3 (1u << 21)
| Ebi signal: A3.
#define | PIO_PC22A_A4 (1u << 22)
| Ebi signal: A4.
#define | PIO_PC23A_A5 (1u << 23)
| Ebi signal: A5.
#define | PIO_PC24A_A6 (1u << 24)
| Ebi signal: A6.
#define | PIO_PC25A_A7 (1u << 25)
| Ebi signal: A7.
#define | PIO_PC26A_A8 (1u << 26)
| Ebi signal: A8.
#define | PIO_PC27A_A9 (1u << 27)
| Ebi signal: A9.
#define | PIO_PC0A_D0 (1u << 0)
| Ebi signal: D0.
#define | PIO_PC1A_D1 (1u << 1)
| Ebi signal: D1.
#define | PIO_PC2A_D2 (1u << 2)
| Ebi signal: D2.
#define | PIO_PC3A_D3 (1u << 3)
| Ebi signal: D3.
#define | PIO_PC4A_D4 (1u << 4)
| Ebi signal: D4.
#define | PIO_PC5A_D5 (1u << 5)
| Ebi signal: D5.
#define | PIO_PC6A_D6 (1u << 6)
| Ebi signal: D6.
#define | PIO_PC7A_D7 (1u << 7)
| Ebi signal: D7.
#define | PIO_PC9A_NANDOE (1u << 9)
| Ebi signal: NANDOE.
#define | PIO_PC10A_NANDWE (1u << 10)
| Ebi signal: NANDWE.
#define | PIO_PC14A_NCS0 (1u << 14)
| Ebi signal: NCS0.
#define | PIO_PC15A_NCS1 (1u << 15)
| Ebi signal: NCS1.
#define | PIO_PA22C_NCS2 (1u << 22)
| Ebi signal: NCS2.
#define | PIO_PC12A_NCS3 (1u << 12)
| Ebi signal: NCS3.
#define | PIO_PC11A_NRD (1u << 11)
| Ebi signal: NRD.
#define | PIO_PC13A_NWAIT (1u << 13)
| Ebi signal: NWAIT.
#define | PIO_PC8A_NWE (1u << 8)
| Ebi signal: NWE.
#define | PIO_PA28C_MCCDA (1u << 28)
| Hsmci signal: MCCDA.
#define | PIO_PA29C_MCCK (1u << 29)
| Hsmci signal: MCCK.
#define | PIO_PA30C_MCDA0 (1u << 30)
| Hsmci signal: MCDA0.
#define | PIO_PA31C_MCDA1 (1u << 31)
| Hsmci signal: MCDA1.
#define | PIO_PA26C_MCDA2 (1u << 26)
| Hsmci signal: MCDA2.
#define | PIO_PA27C_MCDA3 (1u << 27)
| Hsmci signal: MCDA3.
#define | PIO_PA24D_PIODC0 (1u << 24)
| Pioa signal: PIODC0.
#define | PIO_PA25D_PIODC1 (1u << 25)
| Pioa signal: PIODC1.
#define | PIO_PA26D_PIODC2 (1u << 26)
| Pioa signal: PIODC2.
#define | PIO_PA27D_PIODC3 (1u << 27)
| Pioa signal: PIODC3.
#define | PIO_PA28D_PIODC4 (1u << 28)
| Pioa signal: PIODC4.
#define | PIO_PA29D_PIODC5 (1u << 29)
| Pioa signal: PIODC5.
#define | PIO_PA30D_PIODC6 (1u << 30)
| Pioa signal: PIODC6.
#define | PIO_PA31D_PIODC7 (1u << 31)
| Pioa signal: PIODC7.
#define | PIO_PA23D_PIODCCLK (1u << 23)
| Pioa signal: PIODCCLK.
#define | PIO_PA15D_PIODCEN1 (1u << 15)
| Pioa signal: PIODCEN1.
#define | PIO_PA16D_PIODCEN2 (1u << 16)
| Pioa signal: PIODCEN2.
#define | PIO_PA6B_PCK0 (1u << 6)
| Pmc signal: PCK0.
#define | PIO_PB13B_PCK0 (1u << 13)
| Pmc signal: PCK0.
#define | PIO_PA17B_PCK1 (1u << 17)
| Pmc signal: PCK1.
#define | PIO_PA21B_PCK1 (1u << 21)
| Pmc signal: PCK1.
#define | PIO_PA18B_PCK2 (1u << 18)
| Pmc signal: PCK2.
#define | PIO_PA31B_PCK2 (1u << 31)
| Pmc signal: PCK2.
#define | PIO_PB3B_PCK2 (1u << 3)
| Pmc signal: PCK2.
#define | PIO_PA9C_PWMFI0 (1u << 9)
| Pwm signal: PWMFI0.
#define | PIO_PA0A_PWMH0 (1u << 0)
| Pwm signal: PWMH0.
#define | PIO_PA11B_PWMH0 (1u << 11)
| Pwm signal: PWMH0.
#define | PIO_PA23B_PWMH0 (1u << 23)
| Pwm signal: PWMH0.
#define | PIO_PB0A_PWMH0 (1u << 0)
| Pwm signal: PWMH0.
#define | PIO_PC18B_PWMH0 (1u << 18)
| Pwm signal: PWMH0.
#define | PIO_PA1A_PWMH1 (1u << 1)
| Pwm signal: PWMH1.
#define | PIO_PA12B_PWMH1 (1u << 12)
| Pwm signal: PWMH1.
#define | PIO_PA24B_PWMH1 (1u << 24)
| Pwm signal: PWMH1.
#define | PIO_PB1A_PWMH1 (1u << 1)
| Pwm signal: PWMH1.
#define | PIO_PC19B_PWMH1 (1u << 19)
| Pwm signal: PWMH1.
#define | PIO_PA2A_PWMH2 (1u << 2)
| Pwm signal: PWMH2.
#define | PIO_PA13B_PWMH2 (1u << 13)
| Pwm signal: PWMH2.
#define | PIO_PA25B_PWMH2 (1u << 25)
| Pwm signal: PWMH2.
#define | PIO_PB4B_PWMH2 (1u << 4)
| Pwm signal: PWMH2.
#define | PIO_PC20B_PWMH2 (1u << 20)
| Pwm signal: PWMH2.
#define | PIO_PA7B_PWMH3 (1u << 7)
| Pwm signal: PWMH3.
#define | PIO_PA14B_PWMH3 (1u << 14)
| Pwm signal: PWMH3.
#define | PIO_PA17C_PWMH3 (1u << 17)
| Pwm signal: PWMH3.
#define | PIO_PB14B_PWMH3 (1u << 14)
| Pwm signal: PWMH3.
#define | PIO_PC21B_PWMH3 (1u << 21)
| Pwm signal: PWMH3.
#define | PIO_PA19B_PWML0 (1u << 19)
| Pwm signal: PWML0.
#define | PIO_PB5B_PWML0 (1u << 5)
| Pwm signal: PWML0.
#define | PIO_PC0B_PWML0 (1u << 0)
| Pwm signal: PWML0.
#define | PIO_PC13B_PWML0 (1u << 13)
| Pwm signal: PWML0.
#define | PIO_PA20B_PWML1 (1u << 20)
| Pwm signal: PWML1.
#define | PIO_PB12A_PWML1 (1u << 12)
| Pwm signal: PWML1.
#define | PIO_PC1B_PWML1 (1u << 1)
| Pwm signal: PWML1.
#define | PIO_PC15B_PWML1 (1u << 15)
| Pwm signal: PWML1.
#define | PIO_PA16C_PWML2 (1u << 16)
| Pwm signal: PWML2.
#define | PIO_PA30A_PWML2 (1u << 30)
| Pwm signal: PWML2.
#define | PIO_PB13A_PWML2 (1u << 13)
| Pwm signal: PWML2.
#define | PIO_PC2B_PWML2 (1u << 2)
| Pwm signal: PWML2.
#define | PIO_PA15C_PWML3 (1u << 15)
| Pwm signal: PWML3.
#define | PIO_PC3B_PWML3 (1u << 3)
| Pwm signal: PWML3.
#define | PIO_PC22B_PWML3 (1u << 22)
| Pwm signal: PWML3.
#define | PIO_PA12A_MISO (1u << 12)
| Spi signal: MISO.
#define | PIO_PA13A_MOSI (1u << 13)
| Spi signal: MOSI.
#define | PIO_PA11A_NPCS0 (1u << 11)
| Spi signal: NPCS0.
#define | PIO_PA9B_NPCS1 (1u << 9)
| Spi signal: NPCS1.
#define | PIO_PA31A_NPCS1 (1u << 31)
| Spi signal: NPCS1.
#define | PIO_PB14A_NPCS1 (1u << 14)
| Spi signal: NPCS1.
#define | PIO_PC4B_NPCS1 (1u << 4)
| Spi signal: NPCS1.
#define | PIO_PA10B_NPCS2 (1u << 10)
| Spi signal: NPCS2.
#define | PIO_PA30B_NPCS2 (1u << 30)
| Spi signal: NPCS2.
#define | PIO_PB2B_NPCS2 (1u << 2)
| Spi signal: NPCS2.
#define | PIO_PA3B_NPCS3 (1u << 3)
| Spi signal: NPCS3.
#define | PIO_PA5B_NPCS3 (1u << 5)
| Spi signal: NPCS3.
#define | PIO_PA22B_NPCS3 (1u << 22)
| Spi signal: NPCS3.
#define | PIO_PA14A_SPCK (1u << 14)
| Spi signal: SPCK.
#define | PIO_PA18A_RD (1u << 18)
| Ssc signal: RD.
#define | PIO_PA20A_RF (1u << 20)
| Ssc signal: RF.
#define | PIO_PA19A_RK (1u << 19)
| Ssc signal: RK.
#define | PIO_PA17A_TD (1u << 17)
| Ssc signal: TD.
#define | PIO_PA15A_TF (1u << 15)
| Ssc signal: TF.
#define | PIO_PA16A_TK (1u << 16)
| Ssc signal: TK.
#define | PIO_PA4B_TCLK0 (1u << 4)
| Tc0 signal: TCLK0.
#define | PIO_PA28B_TCLK1 (1u << 28)
| Tc0 signal: TCLK1.
#define | PIO_PA29B_TCLK2 (1u << 29)
| Tc0 signal: TCLK2.
#define | PIO_PA0B_TIOA0 (1u << 0)
| Tc0 signal: TIOA0.
#define | PIO_PA15B_TIOA1 (1u << 15)
| Tc0 signal: TIOA1.
#define | PIO_PA26B_TIOA2 (1u << 26)
| Tc0 signal: TIOA2.
#define | PIO_PA1B_TIOB0 (1u << 1)
| Tc0 signal: TIOB0.
#define | PIO_PA16B_TIOB1 (1u << 16)
| Tc0 signal: TIOB1.
#define | PIO_PA27B_TIOB2 (1u << 27)
| Tc0 signal: TIOB2.
#define | PIO_PC25B_TCLK3 (1u << 25)
| Tc1 signal: TCLK3.
#define | PIO_PC28B_TCLK4 (1u << 28)
| Tc1 signal: TCLK4.
#define | PIO_PC31B_TCLK5 (1u << 31)
| Tc1 signal: TCLK5.
#define | PIO_PC23B_TIOA3 (1u << 23)
| Tc1 signal: TIOA3.
#define | PIO_PC26B_TIOA4 (1u << 26)
| Tc1 signal: TIOA4.
#define | PIO_PC29B_TIOA5 (1u << 29)
| Tc1 signal: TIOA5.
#define | PIO_PC24B_TIOB3 (1u << 24)
| Tc1 signal: TIOB3.
#define | PIO_PC27B_TIOB4 (1u << 27)
| Tc1 signal: TIOB4.
#define | PIO_PC30B_TIOB5 (1u << 30)
| Tc1 signal: TIOB5.
#define | PIO_PA4A_TWCK0 (1u << 4)
| Twi0 signal: TWCK0.
#define | PIO_PA3A_TWD0 (1u << 3)
| Twi0 signal: TWD0.
#define | PIO_PB5A_TWCK1 (1u << 5)
| Twi1 signal: TWCK1.
#define | PIO_PB4A_TWD1 (1u << 4)
| Twi1 signal: TWD1.
#define | PIO_PA9A_URXD0 (1u << 9)
| Uart0 signal: URXD0.
#define | PIO_PA10A_UTXD0 (1u << 10)
| Uart0 signal: UTXD0.
#define | PIO_PB2A_URXD1 (1u << 2)
| Uart1 signal: URXD1.
#define | PIO_PB3A_UTXD1 (1u << 3)
| Uart1 signal: UTXD1.
#define | PIO_PA8A_CTS0 (1u << 8)
| Usart0 signal: CTS0.
#define | PIO_PA7A_RTS0 (1u << 7)
| Usart0 signal: RTS0.
#define | PIO_PA5A_RXD0 (1u << 5)
| Usart0 signal: RXD0.
#define | PIO_PA2B_SCK0 (1u << 2)
| Usart0 signal: SCK0.
#define | PIO_PA6A_TXD0 (1u << 6)
| Usart0 signal: TXD0.
#define | PIO_PA25A_CTS1 (1u << 25)
| Usart1 signal: CTS1.
#define | PIO_PA26A_DCD1 (1u << 26)
| Usart1 signal: DCD1.
#define | PIO_PA28A_DSR1 (1u << 28)
| Usart1 signal: DSR1.
#define | PIO_PA27A_DTR1 (1u << 27)
| Usart1 signal: DTR1.
#define | PIO_PA29A_RI1 (1u << 29)
| Usart1 signal: RI1.
#define | PIO_PA24A_RTS1 (1u << 24)
| Usart1 signal: RTS1.
#define | PIO_PA21A_RXD1 (1u << 21)
| Usart1 signal: RXD1.
#define | PIO_PA23A_SCK1 (1u << 23)
| Usart1 signal: SCK1.
#define | PIO_PA22A_TXD1 (1u << 22)
| Usart1 signal: TXD1.
#define | PIO_PC17B_CTS2 (1u << 17)
| Usart2 signal: CTS2.
#define | PIO_PC16B_RTS2 (1u << 16)
| Usart2 signal: RTS2.
#define | PIO_PC9B_RXD2 (1u << 9)
| Usart2 signal: RXD2.
#define | PIO_PC14B_SCK2 (1u << 14)
| Usart2 signal: SCK2.
#define | PIO_PC10B_TXD2 (1u << 10)
| Usart2 signal: TXD2.

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines