<?xml version="1.0" encoding="iso-8859-1"?>

<flash_device>
  <exe>$TOOLKIT_DIR$\config\flashloader\ATMEL\SAM3S16\internalflash-sam3s16.out</exe>
  <flash_base>0x400000</flash_base>
  <page>2048</page>
  <block>32 0x8000</block>
  <macro>$TOOLKIT_DIR$\config\flashloader\ATMEL\resources\sam3s16_flash.mac</macro>
  <args_doc>[--flash] specifies the flash loader program internal flash.
[--boot] is given, it will boot from flash after it is programmed.
</args_doc>
</flash_device>

