SAM3S8/SD8 Software Package: _SBCInquiry Struct Reference

SAM3S8/SD8 Software Package 1.2
Data Fields

# _SBCInquiry Struct Reference
[USB Massstorage Device Driver]

## Data Fields

unsigned char | bOperationCode
unsigned char | isEVPD:1
unsigned char | bReserved1:7
unsigned char | bPageCode
unsigned char | pAllocationLength [2]
unsigned char | bControl

## Detailed Description

Definition at line 358 of file SBC.h.

## Field Documentation

unsigned char _SBCInquiry::bControl

0x00

Definition at line 365 of file SBC.h.

unsigned char _SBCInquiry::bOperationCode

0x12 : SBC_INQUIRY

Definition at line 360 of file SBC.h.

unsigned char _SBCInquiry::bPageCode

Specifies the VPD to return

Definition at line 363 of file SBC.h.

unsigned char _SBCInquiry::bReserved1

Reserved bits

Definition at line 361 of file SBC.h.

unsigned char _SBCInquiry::isEVPD

Type of requested data

Definition at line 361 of file SBC.h.

unsigned char _SBCInquiry::pAllocationLength[2]

Size of host buffer

Definition at line 364 of file SBC.h.

The documentation for this struct was generated from the following file:

- libraries/usb/include/SBC.h

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines