SAM3S8/SD8 Software Package: Audio Device IDs required by driver

SAM3S8/SD8 Software Package 1.2
Defines

# Audio Device IDs required by driver
[USB Device Speaker Phone Driver]

Collaboration diagram for Audio Device IDs required by driver:

## Defines

#define | AUDD_ID_SpeakerIT 0x01
#define | AUDD_ID_SpeakerOT 0x02
#define | AUDD_ID_SpeakerFU 0x03
#define | AUDD_ID_MicrophoneIT 0x04
#define | AUDD_ID_MicrophoneOT 0x05
#define | AUDD_ID_MicrophoneFU 0x06

## Detailed Description

The driver uses following fixed entity IDs, use them to define your descriptor. AUDD_ID_SpeakerIT AUDD_ID_SpeakerOT AUDD_ID_SpeakerFU AUDD_ID_MicrophoneIT AUDD_ID_MicrophoneOT AUDD_ID_MicrophoneFU

## Define Documentation

#define AUDD_ID_MicrophoneFU 0x06

Microphone feature unit ID

Definition at line 80 of file AUDDSpeakerPhone.h.

#define AUDD_ID_MicrophoneIT 0x04

Microphone input terminal ID

Definition at line 76 of file AUDDSpeakerPhone.h.

#define AUDD_ID_MicrophoneOT 0x05

Microphone output terminal ID

Definition at line 78 of file AUDDSpeakerPhone.h.

#define AUDD_ID_SpeakerFU 0x03

Speaker feature unit ID

Definition at line 74 of file AUDDSpeakerPhone.h.

#define AUDD_ID_SpeakerIT 0x01

Speaker input terminal ID

Definition at line 70 of file AUDDSpeakerPhone.h.

#define AUDD_ID_SpeakerOT 0x02

Speaker output terminal ID

Definition at line 72 of file AUDDSpeakerPhone.h.

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines