SAM3S8/SD8 Software Package: _SBCTestUnitReady Struct Reference

SAM3S8/SD8 Software Package 1.2
Data Fields

# _SBCTestUnitReady Struct Reference
[USB Massstorage Device Driver]

SBCTestUnitReady Data structure for the TEST UNIT READY command. More...

`#include <libraries/usb/include/SBC.h>`

## Data Fields

unsigned char | bOperationCode
unsigned char | pReserved1 [4]
unsigned char | bControl

## Detailed Description

SBCTestUnitReady Data structure for the TEST UNIT READY command.

See also:
  spc4r06.pdf - Section 6.34 - Table 192

Definition at line 510 of file SBC.h.

## Field Documentation

unsigned char _SBCTestUnitReady::bControl

0x00

Definition at line 514 of file SBC.h.

unsigned char _SBCTestUnitReady::bOperationCode

0x00 : SBC_TEST_UNIT_READY

Definition at line 512 of file SBC.h.

unsigned char _SBCTestUnitReady::pReserved1[4]

Reserved bits

Definition at line 513 of file SBC.h.

The documentation for this struct was generated from the following file:

- libraries/usb/include/SBC.h

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines