SAM3S8/SD8 Software Package: _S_ccid_bulk_out_header Struct Reference

SAM3S8/SD8 Software Package 1.2
Data Fields

# _S_ccid_bulk_out_header Struct Reference
[USB CCID Device Driver]

## Data Fields

unsigned char | bMessageType
unsigned long | wLength
unsigned char | bSlot
unsigned char | bSeq
unsigned char | bSpecific_0
unsigned char | bSpecific_1
unsigned char | bSpecific_2
unsigned char | APDU [ABDATA_SIZE]

## Detailed Description

Definition at line 136 of file cciddriver.h.

## Field Documentation

unsigned char _S_ccid_bulk_out_header::APDU[ABDATA_SIZE]

Application Protocol Data Unit

Definition at line 150 of file cciddriver.h.

unsigned char _S_ccid_bulk_out_header::bSeq

Sequence number for command.

Definition at line 144 of file cciddriver.h.

unsigned char _S_ccid_bulk_out_header::bSlot

Identifies the slot number for this command

Definition at line 142 of file cciddriver.h.

unsigned char _S_ccid_bulk_out_header::bSpecific_0

specific register

Definition at line 146 of file cciddriver.h.

unsigned long _S_ccid_bulk_out_header::wLength

Message-specific data length

Definition at line 140 of file cciddriver.h.

The documentation for this struct was generated from the following file:

- libraries/usb/device/ccid/cciddriver.h

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines