Information Center for ARM - EXAMPLE PROJECTS

## Information Center for ARM

## Flashloader for ATMEL

## ssc_pdc_audio

This program plays a WAV file pre-loaded into the sram. The sample WAV file can be found in the same directory of main.c. The audio stream is sent through the SSC interface connected to the WM8731, enabling the sound to be audible using a pair of headphones. Since the WM8731 DAC requires that it be feeded a master clock multiple of the sample rate, it is difficult to handle any WAV file. As such, this example application is limited to playing files with the following format: - Format: WAV - Sample rate: 8 kHz - Bits Per Sample: 16 - Channels: 2 (stereo)