SAM3S8/SD8 Software Package: examples_usb/usb_iad_cdc_cdc/device_descriptor.c File Reference

SAM3S8/SD8 Software Package 1.2
Defines | Variables

# device_descriptor.c File Reference

`#include "board.h"`
`#include <include/USBD_Config.h>`
`#include "DUALCDCDDriver.h"`

Go to the source code of this file.

## Defines

#define | CDCD_Descriptors_NOTIFICATION0 3
| Address of the CDC0 interrupt-in endpoint.
#define | CDCD_Descriptors_DATAIN0 2
| Address of the CDC0 bulk-in endpoint.
#define | CDCD_Descriptors_DATAOUT0 1
| Address of the CDC0 bulk-out endpoint.
#define | CDCD_Descriptors_NOTIFICATION1 6
| Address of the CDC1 interrupt-in endpoint.
#define | CDCD_Descriptors_DATAIN1 5
| Address of the CDC1 bulk-in endpoint.
#define | CDCD_Descriptors_DATAOUT1 4
| Address of the CDC1 bulk-out endpoint.
#define | DUALCDCDDriverDescriptors_PRODUCTID 0x6133
| Device product ID.
#define | DUALCDCDDriverDescriptors_VENDORID 0x03EB
| Device vendor ID (Atmel).
#define | DUALCDCDDriverDescriptors_RELEASE 0x0003
| Device release number.
#define | MIN(a, b) ((a < b) ? a : b)
| Returns the minimum between two values.

## Variables

const USBDDriverDescriptors | dualcdcdDriverDescriptors
| List of descriptors required by an USB audio speaker device driver.

## Detailed Description

Definition in file device_descriptor.c.

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines